Versioning Remie\_Morse

V1.0.0

Initial PCB project

V1.0.1

* Mistake footprint filter FLT DLF162500LT-5028A1: switched pin 3/4.. Realized this after bad BLE performance
* Mistake with removing GND layer on layer 2 and 3
* Remove the open drain resistor on INT (for iam20680), push-pull performs better
* Added overlay markings for iam20680 and max15462
* Added polarity marking for wurth LED
* Added USB power and UART over USB

Git tag v1.0.x

Git push origin tag